Data/hora: 23/09/2024 18:43:32

Biblioteca(s): 	Embrapa Agroindústria de Alimentos.	
Data corrente: 	18/12/2017	
Data da última atualização: 	12/06/2024	
Autoria: 	SANTOS JUNIOR, L. A.; LIMA, E. M. B.; THIRÉ, R. M. S. M.; SILVA, A. L. N.	
Afiliação: 	L. A. Santos Junior, UFRJ; EDLA MARIA BEZERRA LIMA, CTAA; Rossana Mara da Silva Moreira Thiré, UFRJ; A. L. N. Silva, UFRJ.	
Título: 	Effect of addition of mango's seed shell (MSS) in green HDPE properties.	
Ano de publicação: 	2017	
Fonte/Imprenta: 	In: INTERNATIONAL CONFERENCE ON NATURAL POLYMERS, BIOPOLYMERS AND BIOMATERIALS, 5., 2017. Rio de Janeiro. Applications from macro to nanoscale. Rio de Janeiro: Synergia Editora : Universidade Federal do Rio de Janeiro, 2017.	
Páginas: 	p. 152.	
Idioma: 	Inglês	
Notas: 	ICNP. Ref. 155. Editores: Fernando Gomes de Souza Junior, Romildo Dias Toledo Filho,  Sabu Thomas.	
Conteúdo: 	The use of by-products from food industry is an important challenge task all around the world. Mango seeds are agro-industrial by-product available in large quantities in tropical countries. They are basically composed of shell and almond. The shell covers the almond, and contains large amounts of cellulose, lignocellulose and lignin [1]. Nowadays, plastics from petroleum are expected to fully decompose in thousands of years. Thus, the development of sustainable products is an alternative for petroleum based materials due to the reduction of carbon dioxide emissions and to generation of a more economic opportunity for the agricultural sector.	
Palavras-Chave: 	HDPE; Pit.	
Thesagro: 	Casca; Manga; Resíduo Orgânico; Semente; Tecnologia de Alimento.	
Thesaurus Nal: 	Food technology; Mangoes; Polyethylene; Seeds.	
Categoria do assunto: 	X Pesquisa, Tecnologia e Engenharia	
Registro original: 	Embrapa Agroindústria de Alimentos (CTAA)	
Exemplares: 	CTAA - (13986-1) - UPC - SP - DD -  -  -  - DIS