Data/hora: 23/06/2024 00:52:00

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	22/12/1999	
Data da última atualização: 	02/04/2007	
Autoria: 	SOUSA, P. L. de; ENGELSBERG, M.; MATOS, M. A.; COLNAGO, L. A.	
Afiliação: 	UFPE-Depto. Fisica; EMBRAPA-CNPDIA.	
Título: 	Measurements of water transport in a gel by Overhauser magnetic resonance imaging.	
Ano de publicação: 	1998	
Fonte/Imprenta: 	Measurement Science and Technology, Bristol, v. 9, n. 12, p. 1982-1988, Dec. 1998.	
Idioma: 	Inglês	
Conteúdo: 	Overhauser imaging in a magnetic field of 16 mT was employed for a study of water transport during the drying process of an agar gel. The data illustrate important aspects of Overhauser imaging, such as the large sensitivity to small changes of local moisture, which may be attainable under appropriate conditions. The non-Fickian nature of the water transport process can be clearly inferred from the measured moisture profiles.	
Palavras-Chave: 	Gel; Moisture content; MRI; Overhauser imaging; Water transport.	
Thesaurus Nal: 	drying; magnetic resonance imaging.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (5044-1) - UPC - SP - -- - PROCI-98.00077 -  - 1998.00077 - DIS