Data/hora: 19/06/2024 21:12:47

Biblioteca(s): 	Embrapa Florestas.	
Data corrente: 	25/10/2018	
Data da última atualização: 	25/10/2018	
Autoria: 	MATTOS, B. D.; GOMES, G. R.; MATOS, M. de; RAMOS, L. P.; MAGALHAES, W. L. E.	
Afiliação: 	Bruno D. Mattos, UFPR; Gustavo R. Gomes, UFPR; Maílson de Matos, UFPR; Luiz P. Ramos, UFPR; WASHINGTON LUIZ ESTEVES MAGALHAES, CNPF.	
Título: 	Consecutive production of hydroalcoholic extracts, carbohydrates derivatives and silica nanoparticles from Equisetum arvense.	
Ano de publicação: 	2018	
Fonte/Imprenta: 	Waste and Biomass Valorization, v. 9, n. 11, p. 1993-2002, Nov. 2018.	
DOI: 	10.1007/s12649-017-9993-y	
Idioma: 	Inglês	
Conteúdo: 	Intelligent strategies should be used in biorefinery processes for the production of different high-value products from the same raw material. Focused on this, the biomass from Equisetum arvense (horsetail) was used for the consecutive production of an extract with medicinal properties, carbohydrate derivatives, heat energy and nanosilica. The biorefinery of horsetail involved a hydroalcoholic extraction, followed by acid hydrolysis and calcination. The yield of the hydroalcoholic extract was 20.2%; however, the yields of monomeric sugars, heat energy and silica varied with the conditions used in each step of the process. High-quality nanosilica could be obtained using mild acid hydrolysis conditions (120 °C, 1 h, H2SO4·2 wt%) followed by calcination at moderated temperature (650 °C); in this case, the yields of co-products were relatively low. However, such yields were increased by changing the hydrolysis temperature to 140 °C but the resulting silica nanoparticles had lower quality.	
Palavras-Chave: 	Biogenic silica; Compostos de açúcares; Furan; Heat energy; Horsetail; Sílica biogênica; Sugars compounds.	
Thesagro: 	Cavalinha; Energia Térmica.	
Thesaurus Nal: 	Equisetum arvense.	
Categoria do assunto: 	X Pesquisa, Tecnologia e Engenharia	
Registro original: 	Embrapa Florestas (CNPF)	
Exemplares: 	CNPF - (56519-1) - UPC - AP - DD -  -  -  - DIS