Data/hora: 16/06/2024 02:42:08

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	28/03/2005	
Data da última atualização: 	28/03/2005	
Autoria: 	MEDEIROS, E. S.; AGNELLI, J. A. M.; CARVALHO, L. H.; MATTOSO, L. H. C.	
Título: 	Comportamento mecânico de compósitos de resina fenólica reforçados por tecidos híbridos de juta e algodão.	
Ano de publicação: 	2003	
Fonte/Imprenta: 	In: CONGRESSO BRASILEIRO DE POLÍMEROS. 7., nov. 2003., Belo Horizonte, MG. Anais... São Carlos: Associação Brasileira de Polímeros, 2003. p. 717-718.	
Idioma: 	Português	
Conteúdo: 	Tensile properties of novolac type phenolic composites reinforced with jute/cotton hybrid woven fabrics were investigated as a function of fiber orientation and roving/fabric characteristics. Scanning electron microscopy (SEM) was carried out to investigate the fiber-matrix adhesion. Results showed that the composite properties are strongly influenced by test direction and rovings/fabric characteristics. The properties anisotropy was shown to increase with test angle and to depend strongly on type/architecture of the fabric used, i.e., jute rovings diameter and relative fiber content. Best overall mechanical properties were obtained for the composites tested along the jute rovings direction. The composites reinforced by hybrid jute/cotton fabrics are suitable for lightweight structural applications.	
Palavras-Chave: 	Compósitos; Fibras; Inflamabilidade; Polímeros.	
Thesagro: 	Resina.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (8762-1) - UPC - SP - -- - PROCI-03.00107 -  - 2003.00107 - DIS