Data/hora: 31/05/2024 12:23:00

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	23/01/2006	
Data da última atualização: 	23/01/2006	
Autoria: 	MEDEIROS, E. S. de; BERNARDES FILHO, R.; MARTINEZ, R. A. de; GREGÓRIO FILHO, R.; MATTOSO, L. H. C.	
Título: 	Atomic force microscopy (AFM) of cured self assembled films.	
Ano de publicação: 	2005	
Fonte/Imprenta: 	In: LATIN AMERICAN SYMPOSIUM ON SCANNING PROBE MICROSCOPY, 3., 2005, Ouro Preto. [Resumos...]. Ouro Preto: SBMN, 2005. 1 CD-ROM.	
Idioma: 	Inglês	
Conteúdo: 	Ultrathin films of conducting polumers are fundamental parts of many devices such as sensors due to many interesting properties which this class of materials exhibits (1-3). The sensoactive properties, i.e., the ability of a given conducting polymer in changing its transducing properties due to the presence of chemical species in the analyte are dependent , on the characteristics of film itself, such as porosity, roughness, thickness, etc.	
Palavras-Chave: 	AFM; Poly(o-ethoxyaniline); Sensors.	
Thesaurus Nal: 	polymers.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (9225-1) - UPC - SP - -- - PROCI-05.00068 -  - 2005.00068 - DIS