Data/hora: 19/06/2024 16:53:48

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 23/01/2006
Data da última atualização: | 23/01/2006
Autoria: | MEDEIROS, E. S. de; AGNELLI, J. A. M.; JOSEPH, K.; CARVALHO, L. H. De. MATTOSO, L. H. C.
Título: | Mechanical properties of phenolic composites reinforced with jute/cotton hybrid fabrics.
Ano de publicação: | 2006
Fonte/Imprenta: | Polymer composites, Brookfield, v.26, n. 1, Feb. 2005. Disponível em: <http://dx.doi.org/10.1002/pc.20063>. Acesso em: 6 jan. 2006.
Idioma: | Inglês
Conteúdo: | Mechanical properties (tensile, flexural, impact, and dynamic mechanical thermal analysis) of novolac type phenolic composites reinforced with jute/cotton hybrid woven fabrics were investigated as a function of fiber orientation and roving/fabric characteristics. Scanning electron microscopy (SEM) was carried out to investigate the fiber-matrix adhesion. Results showed that the composite properties are strongly influenced by test direction and rovings/fabric characteristics.
Palavras-Chave: | Fiber-matrix; Scaning electron microscopy; SEM.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (9224-1) - UPC - SP - -- - PROCI-05.00067 -  - 2005.00067 - DIS