Data/hora: 11/06/2024 00:14:11

Biblioteca(s): 	Embrapa Clima Temperado.	
Tipo da produção científica: 	Artigo em Periódico Indexado	
Circulação/Nível: 	A - 2	
Data corrente: 	08/10/2020	
Data da última atualização: 	08/10/2020	
Autoria: 	BUENO, M. V.; CAMPOS, A. D. S. de; SILVA, J. T. da; MASSEY, J.; TIMM, L. C.; FARIA, L. C.; ROEL, A.; PARFITT, J. M. B.	
Afiliação: 	MARCOS VALLE BUENO, UFPEL; ALEXSSANDRA DAYANE SOARES DE CAMPOS, UFPEL; JAQUELINE TROMBETTA DA SILVA, UFPEL; JOSEPH MASSEY, USDA AGRICULTURAL RESEARCH SERVICE; LUIS CARLOS TIMM, UFPEL; LESSANDRO COLL FARIA, UFPEL; ÁLVARO ROEL, NATIONAL INSTITUTE OF AGRICULTURAL RESEARCH OF URUGUAY; JOSE MARIA BARBAT PARFITT, CPACT.	
Título: 	Improving the drainage and irrigation efficiencyof lowland soils: land-formingoptions for southern Brazil.	
Ano de publicação: 	2020	
Fonte/Imprenta: 	Journal of Irrigation and Drainage Engineering, v. 146, n. 8, 04020019, Aug. 2020.	
Páginas: 	8 p.	
Idioma: 	Inglês	
Conteúdo: 	Land leveling is used to correct soil surface irregularities to improve surface drainage and irrigation. It also makes the area moremanageable for an array of agricultural activities such as planting and harvesting. The objective of this work was to evaluate two designs ofland forming, one aimed at optimizing drainage and the other at optimizing surface irrigation, using fields with reliefs typical of the lowlandsof southern Brazil. Seven commercial rice fields, ranging in size from 7 to 26 ha, were randomly selected and digital elevation designsgenerated for each. Land-leveling projects were developed using three designs: uniform slope (US) (control), land forming?drainage(LFD), and land forming?irrigation (LFI). Performance comparisons between the designs were evaluated through impacts on soil movement(SM), maximum cut in 99% of the area (MC), cumulative length of levees (LL), and total number of levees (NL). Results indicate that bothLFD and LFI designs would reduce costs and require less soil disturbance compared to leveling to uniform slopes. LFD would require lesssoil movement and lower maximum cuts than LFI. However, LFI would reduce the lengths and numbers of rice levees that could have long-term economic and agronomic benefits not captured in these analyses. These results demonstrate that all land-leveling and land-formingalternatives should be thoroughly examined before undertaking field operations. Study outcomes will be useful to engineers and producers inevaluating options to improve the agricultural productivity of lowlands in southern Brazil, a region of national and international significance.	
Thesagro: 	Agricultura de Precisão; Drenagem; Nivelamento da Terra; Solo Hidromórfico.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Clima Temperado (CPACT)	
Exemplares: 	CPACT - (21662-1) - UPC - AP - DD -  -  -  - DIS