Data/hora: 02/06/2024 00:06:09

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 22/12/1999
Data da última atualização: | 09/03/2010
Autoria: | CARVALHO, A. A.; MASCARENHAS, S.; PAULA, M. H. de.
Afiliação: | UNESP-Campus de Ilha Solteira; EMBRAPA-CNPDIA.
Título: | Calibration of a photoacoustical radiation dosimeter.
Ano de publicação: | 1988
Fonte/Imprenta: | In: INTERNATIONAL SYMPOSIUM ON RADIATION PHYSICS, 4., Oct. 1988, São Paulo, SP. Book of abstracts... São Paulo: [s.n.], 1988.
Páginas: | p.II-27.
Idioma: | Inglês
Conteúdo: | We propose a methodology for calibration of a photoacoustical radiation dosimeter (PARD) which doesn´t require the calibration of its response in a known field of ionizing radiation. The PARD calibration procedure is based on the determination of the photoacoustical dosimeter cell responsivities in the following experimental conditions...
Palavras-Chave: | PARD; photoacoustical.
Thesaurus Nal: | calibration.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (5162-1) - UPC - SP - -- - PROCI-88.00008 -  - 1988.00008 - DIS