Data/hora: 20/06/2024 01:47:53

Biblioteca(s): 	Embrapa Suínos e Aves.	
Tipo da produção científica: 	Artigo em Anais de Congresso	
Data corrente: 	23/05/2016	
Data da última atualização: 	22/02/2017	
Autoria: 	PRANDINI, J. M.; SILVA, M. L. B. da; MEZZARI, M. P.; MICHELON, W.; PIROLLI, M.; SOARES, H. M.	
Afiliação: 	JEAN MICHEL PRANDINI, UFSC; MARCIO LUIS BUSI DA SILVA, CNPSA; MELISSA PAOLA MEZZARI, UNOESC; WILLIAN MICHELON, UFSC; MATEUS PIROLLI, UFSC; HUGO MOREIRA SOARES, UFSC.	
Título: 	Use of swine waste-derived biogas to enhance microalgae productivity.	
Ano de publicação: 	2015	
Fonte/Imprenta: 	In: LATIN AMERICAN CONGRESS, 4., 2015, Florianópolis. Anais... Florianópolis: UFSC, 2015. Disponível on line. SOLABIAA.	
Idioma: 	Inglês	
Conteúdo: 	The effects of swine wastewater-derived biogas on microalgae productivity were determined. Experiments were conducted in a closed photobioreactor containing digestate effluent as culturing media and biogas in the headspaceas source of CO2. Experiments were carried out under mixothrophic and autothrophic conditions. Results showed that autotrophic growth rate (0.6 d-1)was twofoldfaster than mixotrophic. Frequent reinjections of biogas containing up to 2,000 ppm of hydrogen sulfide was not inhibitory to microalgae growth. The rapid removal of H2S in the system suggests photobioreactors can be an interesting alternative to biogas purification. A model to estimate microalgae productivity based on the amount of available CO2, inorganic and organic carbon was developedand showed good data fit correlation (r²= 0.99).	
Palavras-Chave: 	CO2; H2S; Swine wastewater.	
Thesaurus Nal: 	biofiltration; microalgae.	
Categoria do assunto: 	--	
URL: 	http://ainfo.cnptia.embrapa.br/digital/bitstream/item/143269/1/final7858.pdf	
Registro original: 	Embrapa Suínos e Aves (CNPSA)	
Exemplares: 	CNPSA - (20624-1) - UPC - AA - DD -  -  -  - DIS