Data/hora: 23/09/2024 17:55:27

Biblioteca(s): 	Embrapa Agricultura Digital.	
Tipo da produção científica: 	Artigo em Anais de Congresso	
Data corrente: 	07/02/2011	
Data da última atualização: 	27/01/2020	
Autoria: 	MAGALHAES, P. S. G.; QUEIROS, L. R.; GADANHA, C. D.	
Afiliação: 	P. S. GRAZIANO MAGALHAES, FEAGRI/UNICAMP; LEONARDO RIBEIRO QUEIROS, CNPTIA; C. D. GADANHA, ESALQ/USP.	
Título: 	Mepiquat chloride application on cotton at variable rate.	
Ano de publicação: 	2010	
Fonte/Imprenta: 	In: INTERNATIONAL CONFERENCE ON PRECISION AGRICULTURE, 10., 2010, Denver. Proceedings... Denver: Denver Tech Center, 2010.	
Páginas: 	Não paginado.	
Idioma: 	Inglês	
Conteúdo: 	Mepiquat chloride (1.1 - dimethylpiperidinium chloride) are used to control excessive vegetative growth in cotton (Gossypium hirsutum L.) broadcast sprayed by ground or air. As proven by previous researches the variability of the cotton plants height in the field is large enough to justify the application of Mepiquat at variable rate. The major advantages of it are: (i) yield increase; (ii) economy of the applied input; (iii) reducing the potential of environmental pollution. The main objective of this project was to develop a prototype device capable to accomplish the application of Mepiquat at variable rate in real time. This project used an equipment previously developed for automatic mapping of the cotton plants height based on ultrasound transducers. An electronic control device for ground sprayers was designed and constructed based on microcontroller PIC, using open source tools as Java, Linux operational system and IDE Netbeans. The device controls the pressure and flow in the spray line and uses Varitarget® nozzles due to its characteristics of linearity of flow and pressure. The calculation of the Mepiquat dosage to be applied is based on the obtained information of the plants heights and the map of previous application. The laboratory results demonstrate the accuracy of the equipment, with low response time considering the commercial sprayers velocity (3 m.s-1 to 5 m.s-1).	
Palavras-Chave: 	Crescimento vegetativo em algodão; Microcontrolador; Open source tools; Software; Sprayer; Varitarget.	
Thesagro: 	Gossypium Hirsutum; Inibidor de Crescimento.	
Thesaurus Nal: 	Mepiquat.	
Categoria do assunto: 	X Pesquisa, Tecnologia e Engenharia	
URL: 	http://ainfo.cnptia.embrapa.br/digital/bitstream/item/26507/1/abstract-244.pdf	
Registro original: 	Embrapa Agricultura Digital (CNPTIA)	
Exemplares: 	CNPTIA - (15553-1) - UPC - AA - DD -  -  -  - DIS