Data/hora: 19/06/2024 15:39:47

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 14/02/2006
Data da última atualização: | 14/02/2006
Autoria: | OLIVEIRA JÚNIOR, O. N.; ZUCOLOTTO, V.; FERREIRA, M.; MATTOSO, L. H. C.; RIUL JÚNIOR, A.
Título: | Nanostructured films employed in sensors.
Ano de publicação: | 2005
Fonte/Imprenta: | In: SUPRAMOLECULAR ENGINEERING OF CONDUCTING MATERIALS, 2005, Safety Harbor, USA. Capítulo de livro. Safety Harbor, USA: Fractal System, 2005.
Idioma: | Inglês
Conteúdo: | An overview is presented of sensors employing nanostructered films obtained with the Langmuir-Blodgett (LB) and layer-by-layer (LbL) techniques as sensing units. The main advantages of such films are highlighted, with examples of high sensitivity and fast response times. Emphasis is also placed on the synergistic combination of distinct materials in the films, in cases where control of molecular architecture is essential for the sensing ability.
Palavras-Chave: | Langmuir-Blodgett Technique; Layer-by-Layer.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (9408-1) - UPC - SP - -- - PROCI-05.00136 -  - 2005.00136 - DIS