Data/hora: 22/06/2024 14:51:54

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	02/03/2005	
Data da última atualização: 	25/04/2008	
Autoria: 	RIUL JÚNIOR, A.; MATTOSO, L. H. C.; MELLO, S. V.; TELLES, G. D.; OLIVEIRA JÚNIOR, O. N.	
Título: 	Langmuir and Langmuir-Blodgett films of parent polyaniline doped with functionalized acids.	
Ano de publicação: 	1995	
Fonte/Imprenta: 	Synthetic Metals, Lausanne, v. 71, p. 2067-2068, 1995.	
Idioma: 	Inglês	
Conteúdo: 	The fabrication of Langmuir and Langmuir-Blodgett (LB) films from high-molecular-weight, doped parent polyaniline is reported. Parent polyaniline was rendered soluble by doping it with functionalized protonic acids (e.g. camphorsulfonic and toluenesulfonic acids) whose counter-ion induces solubility in low boiling point solvents such as chloroform. Condensed monolayers with high collapse pressures (above 30 mN/m) were obtained when an acidic subphase was used. The monolayers could be readily transferred onto hydrophilic substrates in lhe form of Z-type Langmuir-Blodgett films, and most importantly with transfer ratios close to 1. Interestingly, the fllms are readily obtained in the doped form and are electroactive. 	
Palavras-Chave: 	Langmuir; LB; Polianilina.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (8696-1) - UPC - SP - -- - PROCI-95.00108 -  - 1995.00108 - DIS