Data/hora: 21/06/2024 04:39:45

Biblioteca(s): | Embrapa Acre.
Data corrente: | 07/07/2017
Data da última atualização: | 16/11/2023
Autoria: | PAPA, D. de A.; CAMARGO, A. P.; FIGUEIREDO, E. O.; RODRIGUEZ, L. C. E.
Afiliação: | DANIEL DE ALMEIDA PAPA, CPAF-Acre; Alexandre Pansini Camargo, Universidade de São Paulo (USP/ESALQ); EVANDRO ORFANO FIGUEIREDO, CPAF-Acre; Luiz Carlos Estraviz Rodriguez, Universidade de São Paulo (USP/ESALQ).
Título: | Planejamento de unidades de gestão diferenciada em projeto de manejo florestal sustentável na Amazônia.
Ano de publicação: | 2017
Fonte/Imprenta: | In: SIMPÓSIO BRASILEIRO DE SENSORIAMENTO REMOTO, 18., 2017, Santos. Anais... Santos: Inpe, 2017.
Páginas: | 6 p.
ISBN: | 978-85-17-00088-1
Idioma: | Português
Conteúdo: | Among the logging methods, the Exploration of Reduced Impact (ERI) is the one that brings most financial benefits to producers and to the environment due to the use of macro and micro forest planning techniques. The limitation of this method is the systematic techniques to planning the area, using analogic X,Y coordinate to locate trees and streams on the inventory process. With low accuracy to represent the physical environment and location of trees in production units results in a low operating efficiency and higher environmental interference. The purpose of this work is to integrate the forest planning considering environmental heterogeneity, integrating GNSS receiver, radar altimetric data (SRTM) and the hydrographic micro zoning. The study was done in Sena Madureira, state of Acre, Brazil From the inventory of 5.992 trees generated a volume raster and from the stream shape could be possible to construct the permanent protection area (APP). With this both information, using raster calculate processes, were created 4 unites of management areas. Each unit of management has differentiated intensive capacity to receive infrastructure of yard, road and skidtrail. The categories are: 0 to 60 volume m ³. ha-1, 60.01 to 90 m ³. ha-1, 90.01 to 120.00 m ³. ha-1 and 120.01 to 150 m ³. ha-1, discounting the areas of environmental protection and hydrography. Adopting additional information as volumetry, APPs and hydrographic micro zoning unit differentiated management of forest management in the Amazon.
Palavras-Chave: | Acre; Amazonia Occidental; Amazônia Ocidental; Exactitud; Exploração de Impacto Reduzido (EIR); Exploration of Reduced Impact (ERI); Explotación forestal; Fazenda Guarujá; Geotécnica; Inventário a 100%; Inventario forestal; Manejo de precisão; Modeflora; Sena Madureira (AC); Silvicultura sustentable; Sistemas de información geográfica; Teledetección; Western Amazon.
Thesagro: | Exploração florestal; Extração da madeira; Impacto ambiental; Inventário florestal; Planejamento florestal; Radar; Sensoriamento remoto; Sistema de informação geográfica.
Thesaurus Nal: | Accuracy; Environmental impact; Forest inventory; Geographic information systems; Logging; Remote sensing; Sustainable forestry.
Categoria do assunto: | K Ciência Florestal e Produtos de Origem Vegetal
URL: | http://ainfo.cnptia.embrapa.br/digital/bitstream/item/161510/1/26345.pdf
Registro original: | Embrapa Acre (CPAF-AC)
Exemplares: | CPAF-AC - (26345-1) - UPC - AA - DD -  -  -  - DIS