Data/hora: 25/06/2024 00:50:36

Biblioteca(s): | Embrapa Acre.
Data corrente: | 26/05/2020
Data da última atualização: | 28/06/2021
Autoria: | SILVA, E. F. da; SILVA, G. F. da; FIGUEIREDO, E. O.; MENDONÇA, A. R. de; SANTANA, C. J. de O.; FIEDLER, N. C.; SILVA, J. P. M.; AGUIAR, M. O.; SANTOS, J. S.
Afiliação: | Evandro Ferreira da Silva, Universidade Federal do Piauí (UFPI); Gilson Fernandes da Silva, Universidade Federal do Espírito Santo; EVANDRO ORFANO FIGUEIREDO, CPAF-AC; Adriano Ribeiro de Mendonça, Universidade Federal do Espírito Santo (UFES); Cesar Junio de Oliveira Santana, Remsoft Solution; Nilton César Fiedler, Universidade Federal do Espírito Santo (UFES); Jeferson Pereira Martins Silva, Universidade Federal do Espírito Santo (UFES); Marcelo Otone Aguiar, Universidade Federal do Espírito Santo (UFES); Jeangelis Silva Santos, Universidade Federal do Espírito Santo (UFES).
Título: | Optimized forest planning: allocation of log storage yards in the Amazonian sustainable forest management area.
Ano de publicação: | 2020
Fonte/Imprenta: | Forest Ecology and Management, v. 472, 118231, Sept. 2020.
ISSN: | 0378-1127
DOI: | https://doi.org/10.1016/j.foreco.2020.118231
Idioma: | Inglês
Conteúdo: | In Amazonian native forest management, forest road infrastructures, such as log storage yards and skid trails, arethe most expensive attributes and are responsible for the significant environmental impacts with selective treefelling. Road optimization is crucial for reducing environmental impacts and production costs and is stronglylinked to the optimal location of storage yards, which are essential to forest road planning. Considering thepresent problem and the current solutions available, this case study aimed to evaluate the efficiency andeventual gains of optimized forest planning (OFP), as compared to traditional forest planning (TFP). The TFPmethod is currently used most frequently by forest companies in the Amazon region. The study area of 126.41 habelongs to the National Forest (NAFO) Saracá-Taquera, Forest Management Unit II (FMU-II), Annual ProductionUnit (APU) 04/2018, and Work Unit (WU) 2. For the analysis, two areas were defined for exploration: thefirstwas explored using the OFP mathematical model (57.75 ha) and the second followed the TFP plan of thecompany (68.66 ha). Plans and executions for both areas were compared. The OFP model significantly reducedthe Euclidean distances between tree and yards, with only 0.23 km difference in the amount of planned forestroads, when compared to TFP. Additionally, OFP demonstrated a higher productivity (trees.h-1and m3.h-1), areduction of skid distance (by an average of 17.16%), and reduced the cost of log skidding (m3 by 25.76%). Thus,this study proved that OFP is a viable solution that can be adopted by companies to increase productivity.
Palavras-Chave: | Amazônia Oriental; Eastern amazon; FLONA Saracá-Taquera; Manejo florestal sustentável; Oriximiná (PA); Pará; Terra Santa (PA).
Thesagro: | Administração Florestal; Produtividade.
Thesaurus Nal: | Amazonia; Economic productivity; Sustainable forestry.
Categoria do assunto: | K Ciência Florestal e Produtos de Origem Vegetal
URL: | http://ainfo.cnptia.embrapa.br/digital/bitstream/item/213269/1/26998.pdf
Registro original: | Embrapa Acre (CPAF-AC)
Exemplares: | CPAF-AC - (26998-1) - UPC - AP - DD -  -  -  - DIS