Data/hora: 12/06/2024 15:38:23

Biblioteca(s): | Embrapa Arroz e Feijão.
Data corrente: | 30/10/2017
Data da última atualização: | 30/10/2017
Autoria: | BRUNO, H. M. S.; NARCISO, M. G.; SILVA, G. O. F.; SOUZA, M. A. A. de; GUIMARÃES, C. M.; PEREIRA, R. C.; LOPES JUNIOR, S.
Afiliação: | HUDSON M. S. BRUNO, bolsista CNPAF; MARCELO GONCALVES NARCISO, CNPAF; G. O. F. SILVA, UFG; MARCO A. A. DE SOUZA, UFG; CLEBER MORAIS GUIMARAES, CNPAF; RUBENS DE CASTRO PEREIRA, CNPAF; SERGIO LOPES JUNIOR, CNPAF.
Título: | Use of thermographic sensors to determine the water status of plants in a controlled environment.
Ano de publicação: | 2017
Fonte/Imprenta: | In: LATIN-AMERICAN CONFERENCE ON PLANT PHENOTYPING AND PHENOMICS FOR PLANT BREEDING, 2., 2017, São Carlos. Proceedings. São Carlos: Embrapa Instrumentação, 2017.
Páginas: | p. 31.
Idioma: | Inglês
Notas: | Editores: Paulo Sérgio de Paula Herrmann Junior, Paulino Ribeiro Villas Boas.
Conteúdo: | The foliar temperature of plants, relative to ambient temperature, can be used to infer the water status of plants. Both in the field (crops) and in greenhouse, infrared temperature sensors can be used or even thermal cameras to measure leaf temperature without contact with plants. For the case of the greenhouse, Embrapa Rice and Beans created a system, called SITIS (Integrated System of Induced Treatment of Stress). This platform automates the planning and execution of plant irrigation in a greenhouse.
Palavras-Chave: | Leaf temperature; Thermal camera.
Thesagro: | Estufa.
Thesaurus Nal: | Ambient temperature; Greenhouses; Sensors (equipment).
Categoria do assunto: | X Pesquisa, Tecnologia e Engenharia
URL: | http://ainfo.cnptia.embrapa.br/digital/bitstream/item/165747/1/CNPAF-2017-p31.pdf
Registro original: | Embrapa Arroz e Feijão (CNPAF)
Exemplares: | CNPAF - (34842-1) - UPC - RA - DD - 2017 -  - 2017 - DIS