Data/hora: 23/09/2024 13:49:21

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	22/12/1999	
Data da última atualização: 	22/12/1999	
Autoria: 	NAIME, J. M.; CRESTANA, S.; CONCIANI, W.; SOARES, M. M.	
Afiliação: 	EMBRAPA-CNPDIA; Escola Tecnica Federal de Mato Grosso; UFMT-Depto. Engenharia Civil.	
Título: 	Portable CAT scanner applied to collapsible soil studies.	
Ano de publicação: 	1996	
Fonte/Imprenta: 	In: INTERNATIONAL CONFERENCE ON PHYSICS AND INDUSTRIAL DEVELOPMENT: BRIDGING THE GAP, 2., July 1996, Belo Horizonte, MG. Abstracts... Belo Horizonte: UFMG, 1996.	
Páginas: 	Ref.PB11.	
Idioma: 	Inglês	
Conteúdo: 	The soil collapse is causing huge losses to the grain procedures of Mato Grosso State. As a result of this phenomenon many silos are showing signals of sinking. The soil collapse means a sudden reduction of soil volume, when submitted to a stress, due to a rise on its soil moisture. The collapse occurs when the soil is non-saturated and its structure is metastable. The temporary stability of the soil can be checked out through the matrix potential and natural cements. In this work, computerized tomography (CT) technique was applied to measure the reduction of voids caused by the soil collapse. The equipment is a portable tomograph developed at the Instrumentation Center of EMBRAPA/CNPDIA-Sao Carlos, SP. The analysis were carried out in soil samples collected after the execution of load tests which simulates the silo building, in conditions of natural humidity and saturated soil. The CT scanner has the following characteristics: it can be carried to the field and the scanning mechanism is bipartite. The equipment can do scannings of soil monoliths and trees. It is constituted of a gamma ray source (137Cs), semiconductor detector (CdTe), mechanical system and microprocessed electronic circuit. The obtained results show that the influence of the collapse extends to only a few centimeters under the sitting element level of silo's foundation. The results mean important data for soil testing related to building construction and also for characterization and modeling how collapsible the soils are.	
Palavras-Chave: 	Colapso; Collapse; Estudo; Mato Grosso (estado); Portable CT scanner; Tomografo portatil.	
Thesagro: 	Solo.	
Thesaurus Nal: 	soil.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (5583-1) - UPC - SP - -- - PROCI-96.00148 -  - 1996.00148 - DIS