Data/hora: 22/06/2024 13:47:24

Biblioteca(s): 	Embrapa Gado de Leite.	
Tipo da produção científica: 	Nota Técnica/Nota Científica	
Data corrente: 	14/02/2017	
Data da última atualização: 	30/01/2023	
Autoria: 	MACHADO, F. S.; TOMICH, T. R.; FERREIRA, A. L.; CAVALCANTI, L. F.; CAMPOS, M. M.; PAIVA, C. A. V.; RIBAS, M. N.; PEREIRA, L. G. R.	
Afiliação: 	FERNANDA SAMARINI MACHADO, CNPGL; THIERRY RIBEIRO TOMICH, CNPGL; A. L. Ferreira; L. F. Cavalcanti, CNPq; Intergado; MARIANA MAGALHAES CAMPOS, CNPGL; CLAUDIO ANTONIO VERSIANI PAIVA, CNPGL; M. N. RIBAS, CNPq; Intergado; LUIZ GUSTAVO RIBEIRO PEREIRA, CNPGL.	
Título: 	Technical note: A facility for respiration measurements in cattle.	
Ano de publicação: 	2016	
Fonte/Imprenta: 	Journal of Dairy Science, v. 99, n. 6, p. 4899-4906, 2016.	
Idioma: 	Inglês	
Conteúdo: 	Abstract A respiration system consisting of 4 climate-controlled chambers and 1 set of flowmeters and analyzers was constructed and validated. Each chamber had volume of 21.10 m3 (3.68 × 2.56 × 2.24 m) and was made from steel with double-glazed windows on either side enabling visual contact between animals. The chambers are independently climate-controlled and can maintain temperature and relative humidity in a range from 5 to 45°C and 30 to 80%, respectively. A flow generator and mass flowmeter continuously pull air from each chamber and a slight negative pressure inside the chamber is ensured. Air from all chambers and ambient air share a common gas analysis and data acquisition system for monitoring O2, CO2, and CH4 concentrations over the measurement period, with the cycle time set to 20 min. Analyzers are regularly calibrated and the chambers have mean recoveries of 99.0 and 98.0% for CO2 and CH4, respectively. The chambers are equipped with infrared cameras and electronic feed and water bins for intake measurements, as well as sensors for monitoring animal position and heart rate. Data acquisition and analysis software is used to calculate the rate of consumption of O2 and production of CO2 and CH4. The dynamic respiration measurements are integrated with feed intake data and other sensors. The daily gas exchanges are estimated by integration to determine methane emission and heat production. We conducted a trial with 12 lactating 3/4 Holstein × 1/4 Gyr crossbred dairy cows (6 multiparous and 6 primiparous) under 2 feeding regimens (ad libitum or restricted) to validate the system. Two 22-h respiration measurements were obtained from each cow. Restricted-fed cows showed lower values for milk yield, methane emission, and heat production compared with ad libitum-fed animals. We found no difference between groups for CH4 produced per kilogram of dry matter intake. Repeatability for CH4 emission and heat production was high (0.97 and 0.92, respectively). The respiration system described herein is a useful tool for measuring the dynamic and accumulated data of heat production, methane emission, and feed intake.	
Palavras-Chave: 	Bioenergetics; Indirect calorimetry.	
Thesaurus Nal: 	energy; methane.	
Categoria do assunto: 	L Ciência Animal e Produtos de Origem Animal	
Registro original: 	Embrapa Gado de Leite (CNPGL)	
Exemplares: 	CNPGL - (23292-1) - UPC - AP - DD -  -  -  - DIS