Data/hora: 24/06/2024 15:01:47

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	18/01/2006	
Data da última atualização: 	18/01/2006	
Autoria: 	BORATO, C. E.; GOY, R.; LEITE, F. L.; VASCONCELOS, C. de; TRINDADE NETO, C. G. da, CAMPANA FILHO, S. P.; PEREIRA, M. R.; FONSECA, J. L. C.; OLIIVEIRA JUNIOR, O. N.; MATTOSO, L. H. C.	
Título: 	Layer-by-layer films of poly(o-ethoxyaniline) and chitosan-oly(methacrylic acid) nanoparticles.	
Ano de publicação: 	2005	
Fonte/Imprenta: 	In: INTERNATIONAL SYMPOSIUM ON ELECTRETS, 12.; 2005, Salvador. Proceedings... Salvador: IEEE, 2005. p. 83-86.	
Idioma: 	Inglês	
Conteúdo: 	Layer-by-layer films have been produced with poly(o-ethoxyaniline), chitosan and chitosan-oly(methacrylic acid) nanoparticles. Because the adsosption of LbL films depends on ionic interactions and H-bonding, optimized conditions had to be established for the growth of multilayer films. Ununsually thick films were obtained ffor POE and CS-PMAA, thus demonstrating the importance of using chitosan in the form of nanoparticles. 	
Palavras-Chave: 	CS-PMAA; LbL films; POEA.	
Thesaurus Nal: 	chitosan.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (9171-1) - UPC - SP - -- - PROCI-05.00015 -  - 2005.00015 - DIS