Data/hora: 22/06/2024 08:21:45

Biblioteca(s): | Embrapa Agricultura Digital.
Data corrente: | 04/04/2002
Data da última atualização: | 04/03/2013
Autoria: | VENDRUSCULO, L. G.; MAGALHÃES, P. S. G.; VIEIRA, S. R.
Afiliação: | LAURIMAR GONCALVES VENDRUSCULO, CNPTIA; Feagri/Unicamp; IAC.
Título: | Strategies for soil sampling and multi-layers maps generation through geostatic tools: Development of a computational system.
Ano de publicação: | 2002
Fonte/Imprenta: | In: WORLD CONGRESS OF COMPUTERS IN AGRICULTURE AND NATURAL RESOURCES, 2002, Iguaçu Falls. Proceedings... Iguaçu Falls: ASAE, 2002.
Páginas: | p. 244-249.
Idioma: | Inglês
Notas: | Evento realizado em Foz do Iguaçu, PR.
Conteúdo: | The growing demand for agricultural land is obliging the productive agents to adopt modern methods and techniques to improve yield. Mapping soil attributes has proved to be an important tools in the productivity analysis process. It is known that different soil properties are established when analyzing patterns of spatial and temporal variability. Geostatistic has been applied in the estimation and mapping of soil attributes in unsampled areas. Nevertheless, unlike classical statistics, the geostatistics takes into account the distance between samples pairs to better explain the variance and to estimative values in not sampled areas. Precision Farming comprises geostatistic and other techniques that deal with a specific management system to each field. The purpose of the precision farming is to increase the production while guaranteeing the environmental quality and waste reduction. The objective of this paper is to describe a computer program based on Windows Interfaces (Borland Delphi), able to elaborate soil maps and to perform the analyses in soil multi-layers through the use of geostatistic tools (Classical statistical calculations, Average and Directional semivariograms. Cross- semivariogram, and Simple Kriging and Cokriging estimation and Jack- knifing calculations). The system is practical to a small number of soil sampling schemes. Field data was used to assess the accuracy between the measured and estimative values.
Palavras-Chave: | Amostragem de solo; Aplicação Delphi; Geoestatística.
Thesagro: | Agricultura de Precisão.
Thesaurus Nal: | Geostatistics; Precision agriculture.
Categoria do assunto: | X Pesquisa, Tecnologia e Engenharia
Registro original: | Embrapa Agricultura Digital (CNPTIA)
Exemplares: | CNPTIA - (8748-1) - UPC - PL - PP - 630.285 - WOR - 2002.00006 - DIS